From d1d50072edabfcb188caad33f570b20e8837f4a4 Mon Sep 17 00:00:00 2001
From: nbd <nbd@3c298f89-4303-0410-b956-a3cf2f4a3e73>
Date: Sat, 4 Aug 2007 11:58:31 +0000
Subject: fix a few overfull hboxes, remove some redundant stuff

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@8341 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/adding.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'docs/adding.tex')

diff --git a/docs/adding.tex b/docs/adding.tex
index b1712ac9d..2b47e6a32 100644
--- a/docs/adding.tex
+++ b/docs/adding.tex
@@ -357,7 +357,7 @@ firmware image and flash is structured. You will find below a commented example
 that covers the case of the device where the bootloader can pass to the kernel its partition plan.
 
 First of all, you need to make your flash map driver be visible in the kernel 
-configuration options, this can be done by editing the file 
+configuration options, this can be done by editing the file \
 \textbf{linux/drivers/mtd/maps/Kconfig}:
 
 \begin{verbatim}
-- 
cgit v1.2.3

