From afb87b33ca6a84890e9080260df97b14c9104667 Mon Sep 17 00:00:00 2001
From: agb <agb@3c298f89-4303-0410-b956-a3cf2f4a3e73>
Date: Wed, 31 Dec 2008 19:09:26 +0000
Subject: [package] hostapd,madwifi: rename agmode option to hwmode. 11a and
 11g aren't the only allowed values

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@13790 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/wireless.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'docs/wireless.tex')

diff --git a/docs/wireless.tex b/docs/wireless.tex
index 0f8781020..bc41b0e05 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -31,7 +31,7 @@ config wifi-iface
 config wifi-device      "wifi0"
     option type         "atheros"
     option channel      "5"
-    option agmode  	"11g"
+    option hwmode	"11g"
 
 config wifi-iface
     option device       "wifi0"
@@ -99,18 +99,18 @@ config wifi-device    wifi device name
     option channel    1-14
     option maxassoc   1-128 (broadcom only)
     option distance   1-n
-    option agmode     11b, 11g, 11a, 11bg (atheros only)
+    option hwmode     11b, 11g, 11a, 11bg (atheros, mac80211)
     option rxantenna  0,1,2 (atheros, broadcom)
     option txantenna  0,1,2 (atheros, broadcom)
 
 config wifi-iface
-    option network  the interface you want wifi to bridge with 
+    option network  the interface you want wifi to bridge with
     option device   wifi0, wifi1, wifi2, wifiN
     option mode     ap, sta, adhoc, monitor, or wds
     option txpower  transmission power in dBm
     option ssid     ssid name
     option bssid    bssid address
-    option encryption none, wep, psk, psk2, wpa, wpa2 
+    option encryption none, wep, psk, psk2, wpa, wpa2
     option key      encryption key
     option key1     key 1
     option key2     key 2
-- 
cgit v1.2.3

