From e6d9c8710c5c27c2249c333b5aa5429a9ef2338b Mon Sep 17 00:00:00 2001
From: florian <florian@3c298f89-4303-0410-b956-a3cf2f4a3e73>
Date: Thu, 26 Feb 2009 14:53:03 +0000
Subject: [package] allow mac80211 devices to be configured to do 802.11s,
 requires iw

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@14669 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/wireless.tex | 10 +++++++++-
 1 file changed, 9 insertions(+), 1 deletion(-)

(limited to 'docs/wireless.tex')

diff --git a/docs/wireless.tex b/docs/wireless.tex
index dd6ec43dd..f1725318f 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -107,7 +107,7 @@ config wifi-device    wifi device name
 config wifi-iface
     option network  the interface you want wifi to bridge with
     option device   wifi0, wifi1, wifi2, wifiN
-    option mode     ap, sta, adhoc, monitor, or wds
+    option mode     ap, sta, adhoc, monitor, mesh, or wds
     option txpower  (deprecated) transmission power in dBm
     option ssid     ssid name
     option bssid    bssid address
@@ -184,6 +184,9 @@ config wifi-iface
             \item \texttt{monitor} \\
                 Monitor mode
 
+	    \item \texttt{mesh} \\
+		Mesh Point mode (802.11s)
+
             \item \texttt{wds} \\
                 WDS point-to-point link
 
@@ -229,6 +232,11 @@ config wifi-iface
 
 \end{itemize}
 
+\paragraph{Mesh Point}
+
+Mesh Point (802.11s) is only supported by some mac80211 drivers. It requires the iw package
+to be installed to setup mesh links. OpenWrt creates mshN mesh point interfaces.
+
 \paragraph{Wireless Distribution System}
 
 WDS is a non-standard mode which will be working between two Broadcom devices for instance
-- 
cgit v1.2.3

