From 17d1b91a9611b9278c926e82c9be938ade02d095 Mon Sep 17 00:00:00 2001
From: florian <florian@3c298f89-4303-0410-b956-a3cf2f4a3e73>
Date: Mon, 11 Aug 2008 21:38:50 +0000
Subject: Add 802.1x client configuration support and corresponding
 documentation (#2069)

git-svn-id: svn://svn.openwrt.org/openwrt/trunk@12283 3c298f89-4303-0410-b956-a3cf2f4a3e73
---
 docs/wireless.tex | 33 +++++++++++++++++++++++++++++++++
 1 file changed, 33 insertions(+)

(limited to 'docs/wireless.tex')

diff --git a/docs/wireless.tex b/docs/wireless.tex
index de764a312..675023385 100644
--- a/docs/wireless.tex
+++ b/docs/wireless.tex
@@ -272,6 +272,39 @@ config wifi-iface
     option key      "<psk for WDS>"
 \end{Verbatim}
 
+\paragraph{802.1x configurations}
+
+OpenWrt supports both 802.1x client and Access Point
+configurations. 802.1x client is only working with
+Atheros or mac80211 drivers. Configuration only
+supports EAP types TLS, TTLS or PEAP.
+
+\subparagraph{EAP-TLS}
+
+\begin{Verbatim}
+config wifi-iface
+    option device         "ath0"
+    option network        lan
+    option ssid           OpenWrt
+    option eap_type       tls
+    option ca_cert        "/etc/config/certs/ca.crt"
+    option priv_key       "/etc/config/certs/priv.crt"
+    option priv_key_pwd   "PKCS#12 passphrase"
+\end{Verbatim}
+
+\subparagraph{EAP-PEAP}
+
+\begin{Verbatim}
+config wifi-iface
+    option device         "ath0"
+    option network        lan
+    option ssid           OpenWrt
+    option eap_type       peap
+    option ca_cert        "/etc/config/certs/ca.crt"
+    option auth           MSCHAPV2
+    option identity       username
+    option password       password
+\end{Verbatim}
 
 \paragraph{Limitations:}
 
-- 
cgit v1.2.3

